

CT-910 imei procedure

1. Open Imei tool first and connect cable to TAB(should be on)



2. Then click on connect and check whether it is connected or not



1. Now enter imei number and click on write IMEI0 imei writing is over

