**How to update software from sdcard**

Preparation

1. Make sure the unused memory of the SD card is more than 512M bytes.
2. Copy the update file(such as “Croma\_20130715.zip”) to root directory of the SD card, then insert the SD card to the phone and install the battery.
3. Make sure that the battery has enough energy. Such as the percentage of battery is more than 30 percent.

Begin to update

1. Enter recovery mode
   1. Press the “volume up” key and “power on” key at the same time until the phone enter recovery mode, which shown as picture-1.
2. Select file to update
   1. Press the “volume up/down” key to select “apply update from sdcard”. Shown as picture-1
   2. Press the “power on” key to confirm the selection, the phone will enter another interface. Shown as picture-2.
   3. Press “volume down” to select the update file (here is “Croma\_20130715.zip”).
   4. Press “power on” to confirm, and the phone begin to update.
   5. The process of update will last more than 1 minute, please wait more patiently. The phone will reboot 3 times automatically during the process. Shown as picture-3, picture-4


Check whether the update is successful

1. After several steps above, the phone is already power on. Please check the last 4 numbers of build number of the phone is consistent to last 4 numbers of the update file(here is 0715).


If they are the same, update successfully. Or, it updates failed, please check which step is wrong.

Contact us


Picture-1



Picture-2



Picture-3



Picture-4

