
Titanium S1 and S5(TBW5931) Download method

**Take notice：S1/S5-----AP and BP need put together then Download。**

First: The AP’s directory of all files are copied to theBP’s directory。


The “Confirm File Replace”windowinthecopying process，pls choose“**YES**”button。




Second、open--target。(**first time open target,after need entry “QPST DOWNLOAD”–by power on and volum down**)


Third、download。


Open the “eMMC Software Download app” menu ofQPST。




1. Remove “Programming Boot Loaders” Check box




2. Click “load XML def…” button，to selectburning software directory “rawprogram0.xml”file

3，Click“Load path def…” button，to selectburning software directory “patch0.xml”file 

4、click：“Qualcomm MMC Storage USB Device”，Activation “Download” button。



5、click “Download” button then downloading.



6，When prompted “write complete” then Download complete（Need to manually reboot）。

